# UWaveGestureLibraryAll

Data are accelerometer recording of eight simple gestures; it was first described in [1].

*UWaveGestureLibraryX* is the x-axis reading only.

*UWaveGestureLibraryY* is the y-axis reading only.

*UWaveGestureLibraryZ* is the z-axis reading only.

*UWaveGestureLibraryAll* is the concatenation of three axes readings.

Train size: 896

Test size: 3582

Missing value: No

Number of classses: 8

Time series length: 945

Data donated by Jiayang Liu (see [1], [2]).

[1] Liu, Jiayang, et al. "uWave: Accelerometer-based personalized gesture recognition and its applications." Pervasive and Mobile Computing 5.6 (2009): 657-675.

[2] http://www.timeseriesclassification.com/description.php?Dataset=UWaveGestureLibraryAll