## openscad/airplane/airplane1

### Image | ### Program | ### Conversation

###
CLIP Score: 27.79

                    scad
    // Helper function to create an ellipse
    module ellipse(a, b, thickness=1) {
        scale([a, b, 1])
            circle(thickness);
    }

    // Main fuselage from side view
    module fuselage() {
        linear_extrude(height=2) {
            polygon(points=[
                [0,0], [0,10], [1,11], [10,12], [25,14], [50,16],
                [75,14], [100,12], [105,11], [106,10], [106,0],
                [105,-1], [100,-3], [75,-4], [50,-4], [25,-4], [10,-3], [1,-1], [0,0]
            ]);
        }
    }

    // Main wings from top view
    module wings() {
        linear_extrude(height=2) {
            polygon(points=[
                [20, 0], [60, 20], [80, 25], [60, 30], [20, 50],
                [15, 45], [35, 30], [15, 20], [20, 0]
            ]);
        }
    }

    // Tail wings from top view
    module tail_wings() {
        linear_extrude(height=2) {
            polygon(points=[
                [10, 0], [30, 10], [35, 10], [35, 15],
                [30, 15], [10, 20], [5, 15], [5, 10], [10, 0]
            ]);
        }
    }

    // Vertical stabilizer from side view
    module vertical_stabilizer() {
        linear_extrude(height=2) {
            polygon(points=[
                [0, 0], [10, 4], [12, 15], [10, 16],
                [0, 14], [0, 0]
            ]);
        }
    }

    // Assemble the airplane parts in 2D
    module airplane() {
        translate([0, 0, 0]) fuselage();
        translate([30, 8, -1]) rotate([90, 0, 0]) wings();
        translate([90, 8, -1]) rotate([90, 0, 0]) tail_wings();
        translate([98, 14, -1]) rotate([90, 0, 0]) vertical_stabilizer();
    }

    // Create a projection from the 3D model to 2D plane
    projection(cut=false) {
        airplane();
    }
                    Please generate a 2D CAD file in OpenSCAD for airplane

    Creating a complete airplane model in 2D isn't straightforward because airplanes are inherently 3-dimensional objects. However, you can generate some basic 2D views such as the top view and side view using OpenSCAD by projecting a simplified 3D model into 2D. Here’s a simple example to get you started:

    ```scad
    // Helper function to create an ellipse
    module ellipse(a, b, thickness=1) {
        scale([a, b, 1])
            circle(thickness);
    }

    // Main fuselage from side view
    module fuselage() {
        linear_extrude(height=2) {
            polygon(points=[
                [0,0], [0,10], [1,11], [10,12], [25,14], [50,16],
                [75,14], [100,12], [105,11], [106,10], [106,0],
                [105,-1], [100,-3], [75,-4], [50,-4], [25,-4], [10,-3], [1,-1], [0,0]
            ]);
        }
    }

    // Main wings from top view
    module wings() {
        linear_extrude(height=2) {
            polygon(points=[
                [20, 0], [60, 20], [80, 25], [60, 30], [20, 50],
                [15, 45], [35, 30], [15, 20], [20, 0]
            ]);
        }
    }

    // Tail wings from top view
    module tail_wings() {
        linear_extrude(height=2) {
            polygon(points=[
                [10, 0], [30, 10], [35, 10], [35, 15],
                [30, 15], [10, 20], [5, 15], [5, 10], [10, 0]
            ]);
        }
    }

    // Vertical stabilizer from side view
    module vertical_stabilizer() {
        linear_extrude(height=2) {
            polygon(points=[
                [0, 0], [10, 4], [12, 15], [10, 16],
                [0, 14], [0, 0]
            ]);
        }
    }

    // Assemble the airplane parts in 2D
    module airplane() {
        translate([0, 0, 0]) fuselage();
        translate([30, 8, -1]) rotate([90, 0, 0]) wings();
        translate([90, 8, -1]) rotate([90, 0, 0]) tail_wings();
        translate([98, 14, -1]) rotate([90, 0, 0]) vertical_stabilizer();
    }

    // Create a projection from the 3D model to 2D plane
    projection(cut=false) {
        airplane();
    }
    ```

    Steps:
    1. **Save the code above in an OpenSCAD file (e.g., `airplane.scad`)**.
    2. **Open the file in OpenSCAD**.
    3. OpenSCAD will render the 2D projection of the airplane model.

    This model is very simplified and intended to give you a starting point. You can expand it with finer details and more realistic proportions.