## openscad/butterfly/butterfly3

### Image | ### Program | ### Conversation

###
CLIP Score: 28.08

                    scad
    // Butterfly Parameters
    wing_scale = 0.8;
    wing_thickness = 0.5;
    body_width = 2;
    body_height = 10;

    // Wing Design
    module wing() {
        scale([wing_scale, 1])
        difference() {
            offset(r=wing_thickness)
            offset(d=-1)
                rotate([0, 0, 120])
                scale([2, 1])
                    circle(5);
            offset(r=wing_thickness-0.25)
            offset(d=-1.25)
                rotate([0, 0, 120])
                    circle(3);
        }
    }

    // Butterfly Design
    module butterfly() {
        // Body
        translate([0, 0]) {
            square([body_width, body_height / 2], center = true);
            translate([-body_width / 4, -body_height / 2])
                square([body_width / 2, body_height / 2], center = true);
        }

        // Wings
        translate([-body_width / 2, body_height / 4])
            rotate([0, 0, -45]) wing();
        translate([body_width / 2, body_height / 4])
            rotate([0, 0, 45]) wing();
        translate([-body_width / 2, -body_height / 4])
            rotate([0, 0, -135]) wing();
        translate([body_width / 2, -body_height / 4])
            rotate([0, 0, 135]) wing();
    }

    // Render Butterfly
    butterfly();
                    Please generate a 2D CAD file in OpenSCAD for butterfly

    Creating a butterfly in OpenSCAD involves designing the wings and body of the butterfly using geometric shapes and combining them. Below is an example of an OpenSCAD script to create a simple 2D butterfly:

    ```scad
    // Butterfly Parameters
    wing_scale = 0.8;
    wing_thickness = 0.5;
    body_width = 2;
    body_height = 10;

    // Wing Design
    module wing() {
        scale([wing_scale, 1])
        difference() {
            offset(r=wing_thickness)
            offset(d=-1)
                rotate([0, 0, 120])
                scale([2, 1])
                    circle(5);
            offset(r=wing_thickness-0.25)
            offset(d=-1.25)
                rotate([0, 0, 120])
                    circle(3);
        }
    }

    // Butterfly Design
    module butterfly() {
        // Body
        translate([0, 0]) {
            square([body_width, body_height / 2], center = true);
            translate([-body_width / 4, -body_height / 2])
                square([body_width / 2, body_height / 2], center = true);
        }

        // Wings
        translate([-body_width / 2, body_height / 4])
            rotate([0, 0, -45]) wing();
        translate([body_width / 2, body_height / 4])
            rotate([0, 0, 45]) wing();
        translate([-body_width / 2, -body_height / 4])
            rotate([0, 0, -135]) wing();
        translate([body_width / 2, -body_height / 4])
            rotate([0, 0, 135]) wing();
    }

    // Render Butterfly
    butterfly();
    ```

    To generate a 2D drawing, you can add `projection(cut = false);` at the beginning of the script to project the 3D shape into 2D space, but since the model is purely 2D in this case, it's unnecessary.

    Simply copy the above script into an OpenSCAD environment and render it to see the butterfly.

    If you have OpenSCAD installed, you can directly render and export the 2D design to various formats such as DXF, SVG, or PNG using the export functions provided within OpenSCAD.