### Asset Description:
AHU: Air Handling Unit: A device used to condition and circulate air as part of a heating, ventilating, and air-conditioning (HVAC) system.

### Conditions:
- AHU Running
- SubType NOT RAS or OAU
- OAT > 25 °F
- (Heating Drained Flag = 0 IF Reporting)
- Outside Air Damper > 10% IF Outside Air Damper Minimum % Not Reporting
- CO2 < 1000 ppm IF Reporting
- Return Air Temperature > Setpoint Temperature
- Heating Valve % > 5%

### How long the conditions were met:
Met for 2 Hours

What underlying factor, as presented in the options, could explain the current asset state?
A. Check the command from the BMS
B. Return fans in manual
C. BMS sequence of operation for heating valve is incorrect
D. Static pressure sensors need calibration, repair or replacement


# Answer

Answer: C. BMS sequence of operation for heating valve is incorrect

Guidance Rationale: 
Given that the AHU is running and the outside air temperature (OAT) is above
25 °F, yet the heating valve percentage is greater than 5% while the return air
temperature exceeds the setpoint, it suggests that heating is being applied
unnecessarily. The CO₂ level is below 1000 ppm, indicating that the ventilation
demand is not a contributing factor, and air quality is within acceptable
bounds. The presence of heat input despite these conditions, sustained over a
2-hour period, strongly points to a control logic issue rather than a mechanical
or sensor fault. 

Option A, checking the command from the BMS, might reveal the
incorrect command but does not address the root cause of why the command is
incorrect. Option B, return fans in manual, does not directly relate to the
heating valve operation. Option D, static pressure sensors needing calibration,
repair, or replacement, could affect airflow but does not directly explain the
heating valve behavior. Therefore, the most plausible explanation is that the
BMS sequence of operation for the heating valve is incorrect (Option C), causing
the heating system to run inefficiently or inappropriately.