### Asset Description:
PDU: Power Distribution Unit: A device used to distribute electrical power to equipment within a data center or other industrial setting. It typically consists of a panel with multiple outlets that can be used to connect power cords from various devices.

### Conditions:
- 50% of 650 KW < Power Input < 80% of 650 KW
- Using custom Segrate Values of 38, 47.5, 608, 950 KVA

### How long the conditions were met:
Met for 3 Hours

From the given options, which one MOST likely corresponds to the observed asset behavior?
A. CRAC units that can be turned off to provide energy savings
B. Fans are off
C. PDU unit is overloaded
D. Logic that is working too quickly not allowing the system to stabilized


# Answer

Answer: C. PDU unit is overloaded

Guidance Rationale: Given the asset is a Power Distribution Unit (PDU) and the power input is sustained between 50% and 80% of 650 kW,
the unit is operating in a high-load range for an extended period of 3 hours. Additionally, the presence of custom Segrate Values (38, 47.5, 608, 950 kVA) indicates that the system is configured with
specific load thresholds or monitoring configurations, likely tied to capacity planning or fault prevention. This combination of sustained high power input and threshold-based configuration implies that the system is
functioning under stress and is likely nearing or exceeding safe operational limits. 

Therefore, the most plausible explanation for the observed behavior is that the PDU unit is overloaded.