### Asset Description:
Cooling Tower: A heat rejection device that cools water or other fluids by transferring heat to the atmosphere. It is commonly used in HVAC systems, power plants, and industrial processes.

### Conditions:
- Run Status = 1
- (Condenser Water Return To Tower Temperature - Condenser Water Supply To Chiller Temperature) < 5 °F

### How long the conditions were met:
Met for 2 Hours

Given what is known about the asset’s conditions, which explanation makes the LEAST sense?
A. Broken Belt
B. Check fans and condenser water pumps
C. Logic issues for the cooling tower


# Answer

Answer: A. Broken Belt

Guidance Rationale: 
Given that the cooling tower is actively running (Run Status = 1), and the
temperature difference between the condenser water return to the tower and the
condenser water supply to the chiller is less than 5 °F, this suggests that heat
rejection is not occurring as efficiently as expected. If the belt were broken,
the cooling tower fan would likely not operate at all, which would contradict
the observed active run status. 

Therefore, a broken belt is an unlikely
explanation. In contrast, checking the fans and condenser water pumps (Option B)
makes more sense as it could indicate inefficiencies in these components that
are causing the reduced heat rejection. Similarly, logic issues for the cooling
tower (Option C) could also be a plausible explanation, as faulty control logic
might lead to suboptimal operation of the cooling tower components. Thus, the
explanation that makes the least sense given the conditions is: "Broken Belt."