
## Asset Description:
AHU: Air Handling Unit: A device used to condition and circulate air as part of a heating, ventilating, and air-conditioning (HVAC) system.

## Conditions:
AHU Running for 4 hours
ABS(Setpoint Temperature - Supply Air Temperature) > 7 °F
SubType NOT MULTI
(Cooling Drained Flag = 1 IF Reporting

## Conditions in Natural Language:
The asset is running for 4 hours and the absolute value of the difference between preset threshold temparature and the supply air temparature
is higher than 7 degrees Fahrenheit and the subtype of the air handling unit is not MULTI (multi zone AHU). it’s a single-zone or simple AHU, 
not a "multi-zone" AHU. Further the cooling drain is drained.


## Asset Description:
AHU: Air Handling Unit: A device used to condition and circulate air as part of a heating, ventilating, and air-conditioning (HVAC) system.

## Conditions:
AHU Running
OAT > 35 °F
Preheat Valve % > 97%

## Conditions in Natural Language:
The asset is running while outside air temperature is greater than 35 Fahrenheit and the preheat valve open percentage in the asset is above 97%


## Asset Description:
Boiler: A closed vessel in which water or other fluid is heated. The heated or vaporized fluid exits the boiler for use in various applications, such as heating, power generation, or industrial processes.

## Conditions:
Boiler Running
Conductivity > 4000 umho (0.004 S)

## Conditions in Natural Language:
The asset is running and the water quality conductivity is greater than 4000 umho 0.004 S



## Asset Description:
AHU: Air Handling Unit: A device used to condition and circulate air as part of a heating, ventilating, and air-conditioning (HVAC) system.

## Asset Description:
AHU: Air Handling Unit: A device used to condition and circulate air as part of a heating, ventilating, and air-conditioning (HVAC) system.

## Conditions:
Supply Fan Status = 1
Subtype NOT VAV
Supply Fan Current < 1 amp

## Conditions in Natural Language:
The Air supply fan is running and the subtype of the Air handling unit is not VAV (Variable Air Volume ) and the supply fan has a Current
usage of less than 1 ampere


## Asset Description:
Pump: A device used to move fluid or gas from one place to another. It can include various types of pumps, such as centrifugal pumps, positive displacement pumps, and diaphragm pumps.

## Conditions:
Pump Running
Pump VFD Speed % > 97%
OAT < 95 °F

## Conditions in Natural Language:
The asset is running and the Variable Frequency Drive (VFD) operation speed is greater than 97 percentage and the 
outside air temperatue is less than 95 Fahrenheit


## Asset Description:
AHU: Air Handling Unit: A device used to condition and circulate air as part of a heating, ventilating, and air-conditioning (HVAC) system.

## Conditions:
AHU Running
OAT < 80 °F
Cooling Valve % > 97%
ABS(Supply Air Temperature Setpoint - Supply Air Temperature) > 3 IF  Setpoint Reporting

## Conditions in Natural Language:
The asset is running while the outside temperatue is less than 80 Fahrenheit and the unit’s cooling valve is nearly fully open ( Cooling Valve is open more than 97% )
and further tha absolute value of the difference between set threshold of air temperature and supply air temperature is greater than 3
Fahrenheit


## Asset Description:
Cooling Tower: A heat rejection device that cools water or other fluids by transferring heat to the atmosphere. It is commonly used in HVAC systems, power plants, and industrial processes.

## Conditions:
ABS(Condenser Water Pressure Difference - Condenser Water Pressure  Difference Setpoint) > 5 PSI
OAT < 95 °F

## Conditions in Natural Language:
The absolute value of the Condenser Water Pressure Difference and the user defined set point for it is above 5 PSI and the outside air temperture is
below 95 Fahrenheit.


## Asset Description:
AHU: Air Handling Unit: A device used to condition and circulate air as part of a heating, ventilating, and air-conditioning (HVAC) system.

## Conditions:
AHU Running
Humidifier Valve % > 97%

## Conditions in Natural Language:
The asset is running and the humidifier valve is nearly fully open ( humidifier Valve is open more than 97% )


## Asset Description:
AHU: Air Handling Unit: A device used to condition and circulate air as part of a heating, ventilating, and air-conditioning (HVAC) system.

## Conditions:
AHU Running
(Heating Valve % > 10%
Heating Drained Flag = 1 IF Reporting
(OAT - Supply Air Temperature Setpoint > 5 °F

## Conditions in Natural Language:
The asset is running and the heating valve is open ( heating Valve is open more than 10% ) and heating is drained and the difference 
between the outside air temperatue and supply air temperatue is higher than 5 Fahrenheit

