--- Phase 4: Overall Analysis Report ---
Analyzed 30 unique (task, scale) combinations.

1. Divergence from Baselines:
   - Energy-Guided differs from Top-1 in 96.67% of cases
   - Energy-Guided differs from Best-Time in 26.67% of cases

2. Energy Savings (vs. Baselines):
   - Avg. relative energy savings vs. Top-1: 44.69%
   - Avg. relative energy savings vs. Best-Time: 1.86%

3. Runtime Penalty (vs. Baselines):
   - Avg. relative runtime change vs. Top-1: -45.33%
   - Avg. relative runtime change vs. Best-Time: +1.11%
--- End of Overall Report ---