question: What are the achievable peak physical layer data rates for a RedCap (reduced capability) device with baseline capabilities in FR1 (frequency range 1) FD-FDD? option 1: ~85 Mbps in DL and ~90 Mbps in UL option 2: ~60 Mbps in DL and ~20 Mbps in UL option 3: ~300 Mbps in DL and ~100 Mbps in UL option 4: ~80 Mbps in DL and ~40 Mbps in UL option 5: ~120 Mbps in DL and ~60 Mbps in UL 