question: What aspect of the URSP rule does the Application Traffic Descriptor from the AF guidance affect? [3GPP Release 18] option 1: Route Selection Descriptor Precedence option 2: URSP Traffic Descriptor option 3: DNN selection component option 4: Location Criteria 