question: How do victim gNBs determine if the atmospheric ducting phenomenon has ceased in the wireless framework? [3GPP Release 18] option 1: By establishing backhaul coordination option 2: By receiving a specific signal from the core network option 3: By analyzing the TDD DL-UL patterns option 4: By measuring the total received power option 5: By not receiving any reference signal sent from aggressors 