question: What are the components of a practical PHY (physical) layer architecture for RSMA (Rate-splitting multiple access)? option 1: Finite constellation modulation schemes, finite length polar codes, and AMC option 2: Gaussian signaling and infinite block length coding option 3: CSIT feedback delay and user mobility option 4: V-BLAST receiver and satellite communications option 5: Joint communications and sensing 