question: In which scenarios does the consumer NF determine new QoS parameters? [3GPP Release 18] option 1: When the Target of Analytics Reporting is 'any UE' option 2: When multiple Network Slice instances are deployed option 3: When the application SLA is not satisfied option 4: When NWDAF provides Service Experience statistics option 5: When AF provides Service Experience Information 