question: What does the SMF do when it receives the enabling request for analytics information exposure from a UE? [3GPP Release 18] option 1: Subscribes to the Analytics ID for the UE option 2: Checks if it has already subscribed to the Analytics ID for other UEs option 3: Unsubscribes from the Analytics ID for the UE option 4: Requests analytics information from the NWDAF option 5: Includes an Accept or Reject to the enabling request 