question: When does the NG-RAN perform NG-RAN paging before reporting the UE's location? [3GPP Release 18] option 1: When the UE is in RRC_CONNECTED state option 2: When the UE is in RRC_INACTIVE state option 3: When the NG-RAN receives Location Reporting Control message indicating single stand-alone report option 4: When the NG-RAN receives Location Reporting Control message indicating continuous reporting option 5: When PSCell reporting is requested and the PSCell ID is known 