question: How is the 5G VN group configuration information delivered to the UE? [3GPP Release 18] option 1: Via the NEF using the Nudm_SDM_Get service operation option 2: Via the UDM using the SM subscription data option 3: Via the PCF using the URSP in the UE Configuration Update procedure option 4: Via the SMF using the AF request and the PCF policies option 5: Via the AMF using the SM subscription data and the Internal Group ID(s) 