question: What is the purpose of the multi-transmission and reception point feature introduced in Rel-16? option 1: To allocate frequency bands dynamically based on traffic demands option 2: To support single-input single-output option 3: To enable multi-hop integrated access and backhaul option 4: To provide power savings for user equipments option 5: To enable simultaneous data transmissions from multiple physically separated base stations 