question: What is the purpose of SIC (successive interference cancellation) in PD-NOMA (power-domain non orthogonal multiple access)? option 1: To allocate power levels based on channel gains option 2: To recover the signal of the desired user from superimposed signals option 3: To perform distributed power control at the user side option 4: To improve the sum-rate performance of NOMA 