question: How does analog over-the-air computing reduce access latency in federated edge learning systems? option 1: By eliminating the need for encoding and decoding processes option 2: By reducing the number of communication rounds for convergence option 3: By improving the spectral efficiency of the system option 4: By minimizing the interference noise in the received signal option 5: By optimizing the computation capabilities of edge devices 