question: What is the purpose of coordinated scheduling in F-RANs? option 1: To decrease interference in the medium access control (MAC) layer option 2: To increase interference in the physical layer option 3: To decrease interference with centralized and distributed manners in the physical layer option 4: To increase the signal to interference plus noise ratio (SINR) threshold 