------
## 最终结论
To solve the problem, we need to determine the minimum possible area of a grid such that a toy robot can execute a given sequence of commands without falling off the grid. We can also insert at most one extra command ('W', 'A', 'S', or 'D') at any position in the sequence to potentially minimize the grid area.

Here's how we can approach the solution:

1. **Calculate Original Bounds**: For each command sequence, calculate the original bounds of movement in terms of maximum and minimum x and y coordinates. This will help us determine the original grid size.

2. **Simulate Insertion of Extra Commands**: For each command sequence, simulate inserting an extra command ('W', 'A', 'S', or 'D') at any position and calculate how this affects the bounds. Specifically:
   - 'W' increases the upper bound of y.
   - 'S' decreases the lower bound of y.
   - 'A' decreases the lower bound of x.
   - 'D' increases the upper bound of x.

3. **Calculate Minimum Area**: For each possible insertion, calculate the resulting grid area and track the minimum area observed.

4. **Output Results**: After processing all sequences, output the minimum possible area for each sequence.

Here's how you can implement this in Python:

```python
def calculate_minimum_area_with_insertion(queries):
    results = []
    for s in queries:
        # Initial position
        x = 0
        y = 0
        
        # Track boundaries
        min_x = max_x = min_y = max_y = 0
        
        # Calculate original boundaries
        for command in s:
            if command == 'W':
                y += 1
            elif command == 'S':
                y -= 1
            elif command == 'A':
                x -= 1
            elif command == 'D':
                x += 1
            
            min_x = min(min_x, x)
            max_x = max(max_x, x)
            min_y = min(min_y, y)
            max_y = max(max_y, y)
        
        # Calculate original area
        original_area = (max_x - min_x + 1) * (max_y - min_y + 1)
        
        # Try inserting extra commands and calculate new areas
        min_area = original_area
        
        # Insert an extra W (move up)
        new_max_y = max_y + 1
        new_area_W = (max_x - min_x + 1) * (new_max_y - min_y + 1)
        min_area = min(min_area, new_area_W)
        
        # Insert an extra S (move down)
        new_min_y = min_y - 1
        new_area_S = (max_x - min_x + 1) * (max_y - new_min_y + 1)
        min_area = min(min_area, new_area_S)
        
        # Insert an extra A (move left)
        new_min_x = min_x - 1
        new_area_A = (max_x - new_min_x + 1) * (max_y - min_y + 1)
        min_area = min(min_area, new_area_A)
        
        # Insert an extra D (move right)
        new_max_x = max_x + 1
        new_area_D = (new_max_x - min_x + 1) * (max_y - min_y + 1)
        min_area = min(min_area, new_area_D)

        results.append(min_area)
    
    return results

# Read input data
T = int(input())
queries = [input().strip() for _ in range(T)]

# Calculate results for each query
minimum_areas = calculate_minimum_area_with_insertion(queries)

# Output results for each query
for area in minimum_areas:
    print(area)
```

This code will read multiple test cases from input, compute the minimum possible grid area for each sequence with at most one additional move inserted, and then print out those minimum areas.