3D-printed crossed-barrel structure. For a crossed-barrel lattice printed with the following geometry: layer/repeat count n={n}, orientation angle theta={theta}°, radius ratio r={r}, wall thickness t={t}. Estimate the mechanical toughness.