# Gyrokinetics Data Generation
Scripts and utilities for generating data with the **GKW** flux tube code.  
GKW code is available on [bitbucket](https://bitbucket.org/gkw)

## Getting Started
We provide an example `input.dat` which can be used as a template to start a run.  
Modify the parameters in this file according to your experiment setup and simulation configuration.


## Parameter Ranges
We specify the ranges for sampling the main parameters:

- **`rlt`($R/L_T$, temperature gradient):** [1, 12]  
- **`rln` ($R/L_n$, density gradient):** [1, 7]  
- **`q` ($q$, safety factor):** [1, 9]  
- **`shat` ($\hat{s}$, magnetic shear):** [0.5, 5]  

Additionally, the **noise amplitude** `amp_init` of the initial condition is varied within **[1e-5, 1e-3]**.
