EDN - Blogs Archives - Page 21 of 1988

Advertisement

Brian Dipert October 9, 2020 1
Blogs Brian's Brain

## A quest for faster upstream bandwidth

Pandemic-induced desires for faster upstream bandwidth were the fundamental basis for this engineer's service upgrade
Majeed Ahmad October 9, 2020 2
Blogs IC Designer's Corner

## Why AMD is acquiring FPGA powerhouse Xilinx

AMD is reportedly acquiring FPGA design house Xilinx to boost its server and data center chip
John Dunn October 8, 2020 7
Blogs Living Analog

## LED street-light designs create safety hazards

We have seen street-lighting technology evolve, but not always to public benefit. These recently-installed LED street lights created a very scary safety
Michael D. Allen October 8, 2020 1
Blogs Tales from the Cube

## Testing a mysterious instrument

A young engineer was given a challenge when a test box, blueprints, and a test procedure landed on his
Jessica MacNeil October 7, 2020 Number of comments0
Blogs Celebrating women's history EDN Moments

## Computer programmer Henriette Avram is born, October 7, 1919

On this day in tech history, computer programmer Henriette Avram, whose work modernized libraries, was
Nitin Dahad October 7, 2020 Number of comments0
Blogs Embedded Insights

## Datafication and edge autonomy: The new IoT manifestations

Datafication and edge autonomy are going to become megatrends in the IoT-driven age of
Rajan Bedi October 5, 2020 Number of comments0
Blogs Out-of-this-World Design

## Re-configure space-grade FPGAs in orbit

Re-programming SRAM and flash-based space-grade FPGAs in-orbit offers flexibility to change functionality and improve system performance in response to changing
Majeed Ahmad October 1, 2020 Number of comments0
Blogs Engineering on Wheels

## 3 basic facts about automotive sensor degradation

Here is what causes sensor degradation in automotive environments, how to measure it, and finally, how engineers can mitigate and compensate sensor

Advertisement

# Looking for
DataSheets?

## Recent Posts

- Light sensor affords UVA detection
- AI models recognize children’s speech
- LED status indication battery charger
- 8.3-Mpixel sensor delivers high dynamic range
- Vibration monitoring sensors are self-powered

## Archives

Archives

## Categories

Categories

Advertisement

Search for:

## Recent Comments

- WStephenWoodward on Precision clamp protects data logger
- eldercosta on Bounceless switching: Aluminum foil to the rescue
- WStephenWoodward on A simple ratiometric technique for measurement of very low resistances
- marshalljbell on A simple ratiometric technique for measurement of very low resistances
- bdipert on Apple’s September event: What the announcements meant

### COMING SOON! Buy From EETimes (notify me)

Fields marked with an * are required
Business Email *
*

- Yes, I would like to receive your free eNewsletters, designed to provide me with the most up-to date information available (I understand I can opt-out at any time)
- Yes, I agree to the use of my personal information in accordance with the EETimes Privacy Policy, and the Terms of Use.
- Yes, I agree that my information may be shared with relevant third parties, who may email me based on my interest in products or services

If you are a human seeing this field, please leave it empty.
This website uses cookies. By continuing to browse it, you are agreeing to our use of cookies More info