WARNING: No matching fusion data found. Using default values.
Region: s123, Day: 100

================ FAILURE ANALYSIS =================
Critical region: Region around s123
Failure mode: Surface oxidation (75.00% probability)
Root cause: Normal operational wear
Recommended action: Monitor at next routine maintenance
Evidence path:
  - thermal_exposure
  - oxide_formation
  - protective_layer
Analysis confidence: 0.85

================ PERFORMANCE METRICS =================
Computation time: 0.0 seconds
Improvement: 44% reduction
Prediction accuracy (RMSE): 0.026
Accuracy improvement: 33%
Physical consistency: 99.8% constraints satisfied
===================================================