### Asset Description:
HXU: An Heat Exchange Unit(HXU) is a dedicated heat exchanger module, often integrated into systems such as chilled-water cooling racks, packaged HVAC units, or data center cooling setups. It enables efficient heat transfer to maintain desired temperature levels while isolating the zones or fluid circuits

### Conditions:
- Heating System Drained Flag = 0
- Heating System Status On
- OAT > 65 °F
- Heating Valve < 5%
- Hot Water Temperature > 90 °F

### How long the conditions were met:
Met for 2 Hours

Considering the conditions described, which option best diagnoses the likely cause?
A. A new leak in the air lines
B. Belts are loose or broken
C. BMS schedule has been changed
D. Faulty bypass valves


# Answer

Answer: D. Faulty bypass valves

Guidance Rationale: 
The Heat Exchange Unit (HXU) is responsible for maintaining
temperature by facilitating efficient heat transfer between isolated fluid
circuits. In this case, the heating system is active (Heating System Status =
On), and the outside air temperature (OAT) is above 65 °F, which suggests that
active heating may not be necessary. Despite this, the hot water temperature is
above 90 °F, while the heating valve remains below 5%, indicating that hot water
is not being delivered effectively to the heat exchange path. This mismatch
strongly points to faulty bypass valves, which may be improperly diverting hot
water away from the intended heating loop. 

The conditions persisting for 2 continuous hours further reinforce this diagnosis as a sustained control or
mechanical issue rather than a transient state. In contrast, a new leak in the air lines (Option A) would 
not directly affect the hot water temperature or valve position, and loose or broken belts (Option B) 
would typically impact mechanical components rather than fluid flow. A change in the BMS schedule
(Option C) might explain the heating system being on, but it would not account
for the discrepancy between the hot water temperature and the heating valve
position. Therefore, the most likely cause is "Faulty bypass valves."