# ChlorineConcentration

This data set was introduced in a PhD thesis by Lei Li (see [1]. It was produced by EPANET, a software application that models the hydraulic and water quality behavior of water distribution piping systems. EPANET can track, in a given water network the water level and pressure in each tank, the water flow in the pipes and the concentration of a chemical species (chlorine in this case) throughout the network within a simulated duration.

Each time series is the measurements of the chlorine concentration level at 166 nodes (pipe junctions). The measurements were taken every 5 minutes over 15 days.

Train size: 467

Test size: 3840

Missing value: No

Number of classses: 3

Time series length: 166

Data donated by Lei Li and Christos Faloutsos (see [1], [2]).

[1] http://www.cs.cmu.edu/~leili/pubs/leili-thesis.pdf

[2] http://www.timeseriesclassification.com/description.php?Dataset=ChlorineConcentration