Defines the reason why the PVC entered/exited the alarmed condition.Defines if the SAC (service affect Condition) is caused/cleared by the Frame Relay network(frAlarmed/frClear), or by the ATM network (aisAlarmed/aisClear,rdiAlarmed/aisClear). The nodefect means no current SAC in either network. This object will be part of the frf8PVCAlarmTRAP.
The number of AAL-5 ARP NAK PDU's that are discarded by the interworking function on this ATM VCC.If the iwf, interworking function receives an ATM ARP with opcode 10 (NAK), the ARP packet is discarde, since FR ARP does not support that opcode.
The Objects associated with the protocols registered on a specific Virtual Circuit.
The statistics entry for the Protocol Table.
Interface index of the Frame Relay service this connection exists on.
DLCI of this connection on the frame relay service.
The protocol(s) registered over this Virtual Circuit.
The number of AAL-5 PDU's received by FRF.8 of this protocol type from ATM to FR network direction.
The number of AAL-5 octets received by FRF.8 of this protocol type from ATM to FR network direction.
The number of AAL-5 PDU's transmitted by FRF.8 of this protocol type from FR to ATM network direction.
The number of AAL-5 octets transmitted by FRF.8 of this protocol type from FR to ATM network direction.
This trap indicates when an interworking PVC has experienced an alarmed condition, either on the ATM network side or Frame Relay side. Also it is generated when the PVC alarmed condition is cleared. It carries the opera tional status of the PVC by the frf8ConnOperStatus as well as the reason why exiting,entering or changing the alarmed state frf8ConnPVCAlarmReason. If the interworking PVC changes its status by a AdminStatus command (active/inactive/testing), causing the frf8ConnOperStatus to change (up/down), this trap will be generated with frf8ConnPVCAlarmReason set to 'nodefect'. This TRAP will give the support to manage defects that might occur in either Frame Relay network or ATM network, even if the PVC Operational Status is already down.